Quick Navigation
| Background
| System Summary
| Motherboard
| Processor
| BIOS
| PCI/AGP Devices
| Memory Modules
| Memory (SMBIOS)
| HDD
| ATAPI
| Storage (ASPI)
| Logical Drives
| USB Devices
| Printers
| Slots (SMBIOS)
| Ports (SMBIOS)
| Network
| Monitor
| Video
| Hardware Monitoring
| Diagnostics
| Software
Background
| Background
| Version | ASTRA32 v.3.00
| URL | www.astra32.com
| Network Name | A2KKV_7
| User Name | kkv1
| Report Date | May 29, 2012
| Report Time | 16:29:59
| OS Version | MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
| Registered To | Sysinfo Lab
| License Type | Professional for 1 computer
System Summary
| Processor
| Processor | AMD Phenom II X3 710 2600 MHz
| CPU Clock | 2611.8 MHz (13.0 x 200.9 MHz)
| Level 1 Cache | 3 x 64 kB + 3 x 64 kB (data+instr.)
| Level 2 Cache | 3 x 512 kB
| Level 3 Cache | 1 x 6144 kB
| Motherboard
| System Name | Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
| Motherboard Vendor | Gigabyte Technology Co., Ltd.
| Board Model | Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
| BIOS Version | Award Modular BIOS v6.00PG
| Chipset Name | AMD 770/780FX/790FX
| Chipset Vendor | ATI Technologies Inc
| Chipset | RX790 GFX Single Slot
| Southbridge Vendor | ATI Technologies Inc
| Southbridge | SB700 LPC host controller
| DMI/SMBIOS Version | 2.4
| Memory
| Memory Size | 2094648 kB (2045.55 MB)
| System Memory | 2046 MB
| Memory Module | 1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
| Memory Module | 1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
| Storage
| Floppy Drive | Floppy 1.44 MB (3.5")
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| HDD Model | Kingston DT 101 II
| HDD Size | 3874 MB (3.78 GB)
| CD/DVD Model | _NEC DVD_RW ND-3550A
| CD/DVD Speed | 48x (Write: 48x)
| CD/DVD Model | CD-W540E
| CD/DVD Speed | 48x (Write: 40x)
| Video
| Monitor Vendor | LG Electronics Inc.
| Monitor Model | LG FLATRON F920P
| Video Chip Vendor | ATI Technologies Inc
| Video Chip | RV770 [Radeon HD 4870]
| Video Memory Size | 512 MB
| Sound
| Sound Chip Vendor | ATI Technologies Inc
| Sound Chip | IXP SB600 High Definition Audio Controller
| AC'97/HDA Codec Name | Realtek ALC888/ALC1200
| Sound Chip Vendor | ATI Technologies Inc
| Sound Chip | HD48x0 audio
| AC'97/HDA Codec Name | ATI R600 HDMI
| Sound Chip Vendor | Creative Labs
| Sound Chip | EMU10K2 Audio Chipset (SB Audigy Series)
| Operating System
| Operating System | MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
| Windows Folder | I:\Windows
| Network
| Network Name | A2KKV_7
| Adapter Vendor | Realtek Semiconductor
| Adapter Name | RTL8168/8111 PCI-E Gigabit Ethernet NIC
| Interface Description | Realtek RTL8168C(P)/8111C(P) Family PCI-E Gigabit Ethernet NIC (NDIS 6.20)
| MAC Address | 00-24-1D-89-15-40
| Interface Description | VMware Virtual Ethernet Adapter for VMnet1
| MAC Address | 00-50-56-C0-00-01
| Interface Description | VMware Virtual Ethernet Adapter for VMnet8
| MAC Address | 00-50-56-C0-00-08
| Ports
| LPT Ports | None
| COM Ports | COM1(03F8h)
Motherboard
| System
| System Vendor | Gigabyte Technology Co., Ltd.
| Product Name | GA-MA770T-UD3P
| Version |
| Serial Number |
| UUID | 303032343144383931353430FFFFFFFF
| Wake-up Type | Power Switch
| SKU Number |
| Family |
| Motherboard
| Motherboard Vendor | Gigabyte Technology Co., Ltd.
| Vendor URL | www.gigabyte.com.tw
| Board Model | Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
| Version |
| Serial Number |
| BIOS Version | Award Modular BIOS v6.00PG
| BIOS Date | 03/11/11
| Chipset Name | AMD 770/780FX/790FX
| Chipset Vendor | ATI Technologies Inc
| Chipset | RX790 GFX Single Slot
| Southbridge Vendor | ATI Technologies Inc
| Southbridge | SB700 LPC host controller
| System Enclosure
| Manufacturer | Gigabyte Technology Co., Ltd.
| Type | Desktop
| Version |
| Serial Number |
| Asset Tag |
| Boot-up State | Unknown
| Power Supply State | Unknown
| Thermal State | Unknown
| Security Status | Unknown
| OEM-defined | 00000000h
CPU
| CPU
| Processor | AMD Phenom II X3 710 2600 MHz
| Coprocessor | Internal
| CPU Clock | 2611.8 MHz
| Level 1 Cache | 3 x 64 kB + 3 x 64 kB (data+instr.)
| Level 2 Cache | 3 x 512 kB
| Level 3 Cache | 1 x 6144 kB
| Code Name | Heka
| Manufacturing Process | 45 nm
| HyperTransport Clock | 2009.1 MHz
| FSB Clock | 200.9 MHz
| Multiplier | 13.0
| Expected Clock | 2600.0 MHz
| Socket Type | Socket AM2+/AM3
| Temperature Core 1 | 39 °C (102 °F)
| Temperature Core 2 | 39 °C (102 °F)
| Temperature Core 3 | 39 °C (102 °F)
| Core Voltage | 1.325 V
| Northbridge Clock | 2009.1 MHz
| Northbridge Voltage | 1.200 V
| Vendor | AuthenticAMD
| Processor Name | AMD Phenom(tm) II X3 710 Processor
| Processor Type | Original OEM Processor
| CPUID | Family: 15, Model: 4, Stepping: 2
| Ext. Family/Model | Family: 1, Model: 0
| CPU Signature | 00100F42h
| Brand ID | Phenom II X3 710 (40A6h)
| Number of Cores | 3
| Logical CPU Count | 3
| Core Stepping | RB-C2
| Family Frequency Range | 2.6-3.0 GHz
| Max TDP | 94.9 Wattes
| Max CPUID Level | 5
| Max ExtCPUID Level | 8000001Bh
| Instruction Set
| Floating-Point Unit On-Chip | Supported
| IA MMX Technology | Supported
| SSE Instruction Set | Supported
| SSE2 Instruction Set | Supported
| SSE3 Instruction Set | Supported
| Supplemental SSE3 Instruction Set | Not Supported
| SSE4.1 Instruction Set | Not Supported
| SSE4.2 Instruction Set | Not Supported
| Advanced Vector Extensions (AVX) | Not Supported
| Advanced Vector Extensions 2 (AVX2) | Not Supported
| FMA Instructions Set | Not Supported
| AES Instructions Set | Not Supported
| Intel Extended Memory 64 Tech. | Not Supported
| Intel Architecture - 64 (IA-64) | Not Supported
| AMD MMX Instruction Extensions | Supported
| AMD 3DNow! Instructions | Supported
| AMD 3DNow! Extensions | Supported
| AMD 3DNow! Prefetch | Supported
| AMD SSE4A Extensions | Supported
| AMD eXtended OPeration (XOP) | Not Supported
| AMD Misaligned SSE | Supported
| AMD64 Architecture | Supported
| Cyrix Extended MMX | Not Supported
| CMPXCHG8 Instruction Supported | Supported
| CMPXCHG16 Instruction Supported | Supported
| Fast System Call | Supported
| Conditional Move Instruction | Supported
| CLFLUSH Insruction Supported | Supported
| Fast Save and Restore | Supported
| Monitor/MWAIT Instructions | Supported
| SYSCALL/SYSRET Instructions | Supported
| LAHF/SAHF Instructions | Supported
| POPCNT Insruction Supported | Supported
| XSAVE Insructions Supported | Not Supported
| OS Supports XSAVE Instructions | Not Supported
| PCLMULQDQ Instruction Supported | Not Supported
| MOVBE Insruction Supported | Not Supported
| F16C Insruction Supported | Not Supported
| RDTSCP Insruction Supported | Supported
| RDRAND Insruction Supported | Not Supported
| (RD/WR)(FS/GS) BASE Instructions | Not Supported
| Bit Manipulation 1 Instructions | Not Supported
| Bit Manipulation 1 Instructions | Not Supported
| Enhanced REP MOVSB/STOSB | Not Supported
| INVPCID Instruction | Not Supported
| XSAVEOPT Instruction | Not Supported
| AMD Fast Save and Restore | Supported
| AMD SKINIT, STGI, DEV Supported | Supported
| AMD Light Weight Profiling (LWP) | Not Supported
| AMD FMA4 Insruction Supported | Not Supported
| AMD TBM Insruction Supported | Not Supported
| Processor Features
| Virtual Mode Extension | Supported
| Debugging Extension | Supported
| Page Size Extension | Supported
| Time Stamp Counter | Supported
| Model Specific Registers | Supported
| Physical Address Extension | Supported
| Machine Check Exception | Supported
| On-chip APIC Hardware Supported | Supported
| Memory Type Range Registers | Supported
| Page Global Enable | Supported
| Machine Check Architecture | Supported
| Page Attribute Table | Supported
| 36-bit Page Size Extension | Supported
| Processor Serial Number | Not Supported
| Debug Store | Not Supported
| 64-bit Debug Store | Not Supported
| Self-Snoop | Not Supported
| Hyper-Threading Technology | Not Supported
| Pending Break Enable | Not Supported
| CPL-Qualified Debug Store | Not Supported
| L1 Context ID | Not Supported
| Send Task Priority Messages | Not Supported
| Direct Cache Access | Not Supported
| Performance Capabilities MSR | Not Supported
| x2APIC Architecture | Not Supported
| Advanced Bit Manipulation | Supported
| OS Visible Workaround | Supported
| Instruction Based Sampling | Supported
| 1-GB Large Page | Supported
| Process Context Identifiers | Not Supported
| Time Stamp Counter Deadline | Not Supported
| Intel Virtualization Technology | Not Supported
| Intel Trusted Execution Technology | Not Supported
| Supervisor Mode Execution Protection | Not Supported
| Hardware Lock Elision | Not Supported
| Restricted Transactional Memory | Not Supported
| AMD Turbo Core Technology | Not Supported
| AMD No-execute Page Protection | Supported
| AMD Secure Virtual Machine | Supported
| AMD Model-Specific Registers | Supported
| AMD Multiprocessing Capable | Not Supported
| AMD CMP Legacy Mode | Supported
| AMD CR8 in Legacy Mode | Supported
| AMD Ext. APIC Register Space | Supported
| AMD Watchdog Timer | Supported
| AMD Translation Cache Extension | Not Supported
| AMD Topology Extensions | Not Supported
| AMD Core Performance Counter Ext. | Not Supported
| AMD NB Performance Counter Ext. | Not Supported
| Power Management
| ACPI Supported | Not Supported
| Thermal Monitor Supported | Not Supported
| Thermal Monitor 2 | Not Supported
| Enhanced SpeedStep Technology | Not Supported
| Digital Thermal Sensor | Not Supported
| Always Running APIC Timer | Not Supported
| Invariant TSC | Supported
| Power Limit Notification | Not Supported
| Extended Clock Modulation Duty | Not Supported
| Package Thermal Management | Not Supported
| Hardware Coordination Feedback | Not Supported
| ACNT2 Capability | Not Supported
| Performance-Energy Bias | Not Supported
| AMD Temperature Sensor | Supported
| AMD Frequency ID Control | Not Supported
| AMD Voltage ID Control | Not Supported
| AMD Thermal Trip | Supported
| AMD Thermal Monitoring | Supported
| AMD Software Thermal Control | Supported
| AMD 100MHz Multiplier Steps | Supported
| AMD Hardware P-State Control | Supported
| AMD Effective Frequency Interface | Not Supported
CPU Cache
| Level 1 Instruction Cache
| Size | 3 x 64 kB
| Associativity | 2-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 32
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 16
| Associativity | full
| Level 1 Data Cache
| Size | 3 x 64 kB
| Associativity | 2-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 48
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 48
| Associativity | full
| Level 2 Cache
| Size | 3 x 512 kB
| Associativity | 16-way
| Lines per Tag | 1
| Line Size | 64 byte
| Instr. TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Data TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Instr. TLB 2/4M Pages |
| Number of Entries | 0
| Associativity | off
| Data TLB 2/4M Pages |
| Number of Entries | 128
| Associativity | 2-way
| Level 3 Cache
| Size | 1 x 6144 kB
| Associativity | 48-way
| Line Size | 64 byte
CPU (SMBIOS)
| Processor
| Processor Vendor | AMD
| Processor Version | AMD Phenom(tm) II X3 710 Processor
| Current Speed | 2600 MHz
| External Clock | 200 MHz
| Voltage | 1.3 V
| Processor Upgrade | ZIF Socket
| Processor Status | CPU Enabled
| Socket Designation | Socket M2
| Processor Type | Central Processor
| Processor Family | AMD Athlon
| Processor ID1 | 00100F42h
| Processor ID2 | 178BFBFFh
| Max Speed | 3200 MHz
| Socket Status | CPU Socket Populated
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 23h
CPU (SMBIOS) Cache
| Level 1 Cache
| Installed Size | 128 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | Internal Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 128 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
| Level 1 Cache
| Installed Size | 128 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | Internal Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 128 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
| Level 3 Cache
| Installed Size | 512 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | External Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 512 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
| Level 2 Cache
| Installed Size | 0 kB
| Operational Mode | Write Through
| Current SRAM Type | Synchronous
| Status | Disabled
| Socket Designation | External Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 1024 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
BIOS
| BIOS
| Motherboard Vendor | Gigabyte Technology Co., Ltd.
| Vendor URL | www.gigabyte.com.tw
| BIOS Version | Award Modular BIOS v6.00PG
| BIOS Date | 03/11/11
| BIOS Copyright | Award Software Inc. - 04/23/90
| Motherboard ID | AMD 770 BIOS for GA-MA770T-UD3P F11
| BIOS ID | 03/11/2011-RX780-SB710-7A66AG05C-00
| BIOS Type | Phoenix Award BIOS v6.00
| Bus Type | ISA/PCI
| Processor | 686
| Chipset | AMD 790FX
| Chipset ID | RX780-SB710
| BIOS Revision | 00
| MP Specification Ver. | 1.4
| MP Table Address | 000Fh:1100h
| Number of CPU/Cores | 3
| DMI/SMBIOS Version | 2.4
| DMI/SMBIOS Structures | 55
| DMI/SMBIOS Address | 000Fh:0100h
| SMBIOS
| BIOS Vendor | Award Software International, Inc.
| BIOS Version | F11
| BIOS Date | 03/11/2011
| BIOS ROM Size | 1024 kB
| Starting Segment | E000h
| Current Language | n|US|iso8859-1
| Number of Languages | 3
| Structure Length | 18h
| Bus Supported
| PCI is Supported | Supported
| AGP is Supported | Not Supported
| USB is Supported | Supported
| ISA is Supported | Supported
| VLBus is Supported | Not Supported
| MCA is Supported | Not Supported
| EISA is Supported | Not Supported
| PC Card is Supported | Not Supported
| Boot Options
| Selectable Boot | Supported
| Boot From CD | Supported
| ATAPI ZIP Drive Boot | Supported
| LS-120 Boot | Supported
| BIOS Boot Specification | Supported
| Boot From PC Card | Not Supported
| Network Service Boot Supported | Not Supported
| I2O Boot | Not Supported
| 1394 Boot | Not Supported
| BIOS Features
| BIOS Characteristics | Supported
| ACPI Supported | Supported
| PnP is Supported | Supported
| APM is Supported | Supported
| ESCD Support | Not Supported
| Enhanced Disk Drive (EDD) | Supported
| BIOS is Upgradeable (Flash) | Supported
| BIOS ROM is Socketed | Supported
| BIOS Shadowing is Allowed | Supported
| Smart Battery Supported | Not Supported
| Targeted Content Distribution | Supported
| UEFI Specification is Supported | Not Supported
| Virtual Machine | Not Supported
| Int 13h - 5.25"/360kB Floppy | Supported
| Int 13h - 5.25"/1.2MB Floppy | Supported
| Int 13h - 3.5"/720kB Floppy | Supported
| Int 13h - 3.5"/2.88MB Floppy | Supported
| Int 5h, Print Screen Service | Supported
| Int 9h, 8042 Keyboard Services | Supported
| Int 14h, Serial Services | Supported
| Int 17h, Printer Services | Supported
| Int 10h, CGA/Mono Video Services | Supported
| Int 13h - Floppy for NEC 9800 | Not Supported
| Int 13h - Floppy for Toshiba | Not Supported
| NEC PC-98 | Not Supported
| Other SMBIOS Structures
| Memory Array Mapped Address (19)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| System Boot Information (32)
| Unknown (188)
| Unknown (190)
| Unknown (192)
| Unknown (194)
| Unknown (196)
| Unknown (198)
PCI/AGP Devices
| Bus: 00h, Device: 00h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (5957h) | RX790 GFX Single Slot
| Subsys Vendor (1002h) | ATI Technologies Inc
| Subsystem ID (5957h) | Unknown
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | E0000000h - FFFFFFFFh
| Hyper Transport Capabilities
| HyperTransport Version | 3.00
| Interface Type | Slave/Primary
| Link 0 Frequency | 2000 MHz
| Link 0 Width In | 16 bits (Current: 16 bits)
| Link 0 Width Out | 16 bits (Current: 16 bits)
| Link 1 Frequency | 200 MHz
| Link 1 Width In | 8 bits (Current: 8 bits)
| Link 1 Width Out | 8 bits (Current: 8 bits)
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1002&DEV_5957&SUBSYS_59571002&REV_00
| Compatible ID | PCI\VEN_1002&DEV_5957&REV_00
| Bus: 00h, Device: 02h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (5978h) | RD790 PCI to PCI bridge (external gfx0 port A)
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | E000h - EFFFh
| Memory Address | FDF00000h - FDFFFFFFh
| Memory Address | D0000000h - DFFFFFFFh
| System IRQ | 18
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 5.0 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard PCI-to-PCI bridge
| Device Class | System
| Device Location | PCI bus 0, device 2, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1002&DEV_5978&SUBSYS_59571002&REV_00
| Compatible ID | PCI\VEN_1002&DEV_5978&REV_00
| Bus: 00h, Device: 0Ah, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (597Fh) | RD790 PCI to PCI bridge (PCIe gpp port F)
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | D000h - DFFFh
| Memory Address | FDE00000h - FDEFFFFFh
| Memory Address | FDB00000h - FDBFFFFFh
| System IRQ | 18
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 5
| Physical Slot Number | 1
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard PCI-to-PCI bridge
| Device Class | System
| Device Location | PCI bus 0, device 10, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1002&DEV_597F&SUBSYS_59571002&REV_00
| Compatible ID | PCI\VEN_1002&DEV_597F&REV_00
| Bus: 00h, Device: 11h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4390h) | SB700 SATA Controller [IDE mode]
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (B002h) | GA-MA770-DS3rev2.0 Motherboard
| Class (01h) | Storage
| SubClass (01h) | IDE
| Revision | 00h
| Interface | 8Fh
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000FF00h - 0000FF07h
| Base I/O Port | 0000FE00h - 0000FE03h
| Base I/O Port | 0000FD00h - 0000FD07h
| Base I/O Port | 0000FC00h - 0000FC03h
| Base I/O Port | 0000FB00h - 0000FB0Fh
| Memory Address | FE02F000h - FE02F3FFh
| System IRQ | 22
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard IDE ATA/ATAPI controllers)
| Device Description | Standard Dual Channel PCI IDE Controller
| Device Class | hdc
| Device Location | PCI bus 0, device 17, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | mshdc.inf
| Service Name | pciide
| Hardware ID | PCI\VEN_1002&DEV_4390&SUBSYS_B0021458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4390&REV_00
| Bus: 00h, Device: 12h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4397h) | SB700 USB OHCI0 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02E000h - FE02EFFFh
| System IRQ | 16
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard OpenHCD USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 18, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbohci
| Hardware ID | PCI\VEN_1002&DEV_4397&SUBSYS_50041458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4397&REV_00
| Bus: 00h, Device: 12h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (4398h) | SB700 USB OHCI1 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02D000h - FE02DFFFh
| System IRQ | 16
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard OpenHCD USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 18, function 1
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbohci
| Hardware ID | PCI\VEN_1002&DEV_4398&SUBSYS_50041458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4398&REV_00
| Bus: 00h, Device: 12h, Function: 02h
| Vendor (1002h) | ATI Technologies Inc
| Device (4396h) | SB700 USB EHCI Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02C000h - FE02C0FFh
| System IRQ | 17
| Interrupt Pin | INTB#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard Enhanced PCI to USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 18, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbehci
| Hardware ID | PCI\VEN_1002&DEV_4396&SUBSYS_50041458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4396&REV_00
| Bus: 00h, Device: 13h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4397h) | SB700 USB OHCI0 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02B000h - FE02BFFFh
| System IRQ | 18
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard OpenHCD USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 19, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbohci
| Hardware ID | PCI\VEN_1002&DEV_4397&SUBSYS_50041458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4397&REV_00
| Bus: 00h, Device: 13h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (4398h) | SB700 USB OHCI1 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02A000h - FE02AFFFh
| System IRQ | 18
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard OpenHCD USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 19, function 1
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbohci
| Hardware ID | PCI\VEN_1002&DEV_4398&SUBSYS_50041458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4398&REV_00
| Bus: 00h, Device: 13h, Function: 02h
| Vendor (1002h) | ATI Technologies Inc
| Device (4396h) | SB700 USB EHCI Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE029000h - FE0290FFh
| System IRQ | 19
| Interrupt Pin | INTB#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard Enhanced PCI to USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 19, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbehci
| Hardware ID | PCI\VEN_1002&DEV_4396&SUBSYS_50041458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4396&REV_00
| Bus: 00h, Device: 14h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4385h) | IXP SB600 SMBUS Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (4385h) | GA-MA770-DS3rev2.0 Motherboard
| Class (0Ch) | Serial
| SubClass (05h) | SMBus Controller
| Revision | 3Ch
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Supported
| Device Resources
| SMBus Port | 0B00h
| Driver
| Driver Status | The device is working properly
| Manufacturer | ATI
| Device Description | ATI I/O Communications Processor SMBus Controller
| Device Class | System
| Device Location | PCI bus 0, device 20, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1002&DEV_4385&SUBSYS_43851458&REV_3C
| Compatible ID | PCI\VEN_1002&DEV_4385&REV_3C
| Bus: 00h, Device: 14h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (439Ch) | SB700 IDE
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5002h) | Unknown
| Class (01h) | Storage
| SubClass (01h) | IDE
| Revision | 00h
| Interface | 8Ah
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000FA00h - 0000FA0Fh
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard IDE ATA/ATAPI controllers)
| Device Description | Standard Dual Channel PCI IDE Controller
| Device Class | hdc
| Device Location | PCI bus 0, device 20, function 1
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | mshdc.inf
| Service Name | pciide
| Hardware ID | PCI\VEN_1002&DEV_439C&SUBSYS_50021458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_439C&REV_00
| Bus: 00h, Device: 14h, Function: 02h
| Vendor (1002h) | ATI Technologies Inc
| Device (4383h) | IXP SB600 High Definition Audio Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (A002h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Slow
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FE024000h - FE027FFFh
| System IRQ | 16
| Interrupt Pin | INTA#
| AC'97/HDA Capabilities
| AC'97/HDA Codec Name | Realtek ALC888/ALC1200
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 0, device 20, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 11-19-2010
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_1002&DEV_4383&SUBSYS_A0021458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4383&REV_00
| Bus: 00h, Device: 14h, Function: 03h
| Vendor (1002h) | ATI Technologies Inc
| Device (439Dh) | SB700 LPC host controller
| Subsys Vendor (1002h) | ATI Technologies Inc
| Subsystem ID (439Dh) | Unknown
| Class (06h) | Bridge
| SubClass (01h) | PCI/ISA
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard ISA bridge
| Device Class | System
| Device Location | PCI bus 0, device 20, function 3
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | msisadrv
| Hardware ID | PCI\VEN_1002&DEV_439D&SUBSYS_439D1002&REV_00
| Compatible ID | PCI\VEN_1002&DEV_439D&REV_00
| Bus: 00h, Device: 14h, Function: 04h
| Vendor (1002h) | ATI Technologies Inc
| Device (4384h) | IXP SB600 PCI to PCI Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 00h
| Interface | 01h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | C000h - CFFFh
| Memory Address | FDD00000h - FDDFFFFFh
| Memory Address | FDC00000h - FDCFFFFFh
| Driver
| Driver Status | The device is working properly
| Manufacturer | ATI
| Device Description | ATI I/O Communications Processor PCI Bus Controller
| Device Class | System
| Device Location | PCI bus 0, device 20, function 4
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_1002&DEV_4384&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1002&CC_060401
| Bus: 00h, Device: 14h, Function: 05h
| Vendor (1002h) | ATI Technologies Inc
| Device (4399h) | SB700 USB OHCI2 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE028000h - FE028FFFh
| System IRQ | 18
| Interrupt Pin | INTC#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Standard OpenHCD USB Host Controller
| Device Class | USB
| Device Location | PCI bus 0, device 20, function 5
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbohci
| Hardware ID | PCI\VEN_1002&DEV_4399&SUBSYS_50041458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_4399&REV_00
| Bus: 00h, Device: 18h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1200h) | K10 [Opteron, Athlon64, Sempron] HyperTransport Configuration
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Hyper Transport Capabilities
| HyperTransport Version | 3.00
| Interface Type | Host/Secondary
| Link 0 Frequency | 2000 MHz
| Link 0 Width In | 16 bits (Current: 16 bits)
| Link 0 Width Out | 16 bits (Current: 16 bits)
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1200&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Bus: 00h, Device: 18h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1201h) | K10 [Opteron, Athlon64, Sempron] Address Map
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 1
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1201&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Bus: 00h, Device: 18h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1202h) | K10 [Opteron, Athlon64, Sempron] DRAM Controller
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1202&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Bus: 00h, Device: 18h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1203h) | K10 [Opteron, Athlon64, Sempron] Miscellaneous Control
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 3
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1203&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Bus: 00h, Device: 18h, Function: 04h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1204h) | K10 [Opteron, Athlon64, Sempron] Link Control
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard host CPU bridge
| Device Class | System
| Device Location | PCI bus 0, device 24, function 4
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_1022&DEV_1204&SUBSYS_00000000&REV_00
| Compatible ID | PCI\VEN_1022&CC_060000
| Bus: 01h, Device: 00h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (9440h) | RV770 [Radeon HD 4870]
| Subsys Vendor (1787h) | Hightech Information System Ltd (Medion??)
| Subsystem ID (2267h) | Unknown
| Class (03h) | Display
| SubClass (00h) | VGA
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | D0000000h - DFFFFFFFh
| Memory Address | FDFE0000h - FDFEFFFFh
| Base I/O Port | 0000EE00h - 0000EEFFh
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 5.0 GB/s (Current: 5.0 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices, Inc.
| Device Description | ATI Radeon HD 4800 Series
| Device Class | Display
| Device Location | PCI bus 1, device 0, function 0
| Driver Provider | Advanced Micro Devices, Inc.
| Driver Version | 8.950.0.0
| Driver Date | 2-14-2012
| Inf File | oem3.inf
| Service Name | amdkmdap
| Hardware ID | PCI\VEN_1002&DEV_9440&SUBSYS_22671787&REV_00
| Compatible ID | PCI\VEN_1002&DEV_9440&REV_00
| Bus: 01h, Device: 00h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (AA30h) | HD48x0 audio
| Subsys Vendor (1787h) | Hightech Information System Ltd (Medion??)
| Subsystem ID (AA30h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FDFFC000h - FDFFFFFFh
| System IRQ | 19
| Interrupt Pin | INTB#
| AC'97/HDA Capabilities
| AC'97/HDA Codec Name | ATI R600 HDMI
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 5.0 GB/s (Current: 5.0 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 1, device 0, function 1
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 11-19-2010
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_1002&DEV_AA30&SUBSYS_AA301787&REV_00
| Compatible ID | PCI\VEN_1002&DEV_AA30&REV_00
| Bus: 02h, Device: 00h, Function: 00h
| Vendor (10ECh) | Realtek Semiconductor
| Device (8168h) | RTL8168/8111 PCI-E Gigabit Ethernet NIC
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (E000h) | GA-EP45-DS5 Motherboard
| Class (02h) | Network
| SubClass (00h) | Ethernet
| Revision | 02h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000DE00h - 0000DEFFh
| Memory Address | FDBFF000h - FDBFFFFFh
| Memory Address | FDBE0000h - FDBEFFFFh
| System IRQ | 18
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 1.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 2.5 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Realtek
| Device Description | Realtek RTL8168C(P)/8111C(P) Family PCI-E Gigabit Ethernet NIC (NDIS 6.20)
| Device Class | Net
| Device Location | PCI bus 2, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 7.2.1127.2008
| Driver Date | 2-26-2008
| Inf File | netrtx64.inf
| Service Name | RTL8167
| Hardware ID | PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_02
| Compatible ID | PCI\VEN_10EC&DEV_8168&REV_02
| Bus: 03h, Device: 06h, Function: 00h
| Vendor (1102h) | Creative Labs
| Device (0004h) | EMU10K2 Audio Chipset (SB Audigy Series)
| Subsys Vendor (1102h) | Creative Labs
| Subsystem ID (2005h) | Unknown
| Class (04h) | Multimedia
| SubClass (01h) | Audio
| Revision | 04h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000CF00h - 0000CF3Fh
| System IRQ | 20
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is disabled (22)
| Manufacturer | Creative Technology, Ltd.
| Device Description | Creative Audigy Audio Processor (WDM)
| Friendly Name | Creative SB Audigy 2 ZS (WDM)
| Device Class | MEDIA
| Device Location | PCI bus 3, device 6, function 0
| Driver Provider | Creative
| Driver Version | 6.0.1.1377
| Driver Date | 3-18-2010
| Inf File | oem2.inf
| Service Name | ctaud2k
| Hardware ID | PCI\VEN_1102&DEV_0004&SUBSYS_20051102&REV_04
| Compatible ID | PCI\VEN_1102&DEV_0004&REV_04
| Bus: 03h, Device: 0Eh, Function: 00h
| Vendor (104Ch) | Texas Instruments (TI)
| Device (8024h) | TSB43AB23 1394a-2000 OHCI PHY/link-layer Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (1000h) | GA-EP45-DS5 Motherboard
| Class (0Ch) | Serial
| SubClass (00h) | Firewire
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FDDFF000h - FDDFF7FFh
| Memory Address | FDDF8000h - FDDFBFFFh
| System IRQ | 22
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Texas Instruments
| Device Description | Texas Instruments 1394 OHCI Compliant Host Controller
| Device Class | 1394
| Device Location | PCI bus 3, device 14, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | 1394.inf
| Service Name | 1394ohci
| Hardware ID | PCI\VEN_104C&DEV_8024&SUBSYS_10001458&REV_00
| Compatible ID | PCI\VEN_104C&DEV_8024&REV_00
Memory Modules
| Memory Slot 1
| Memory Type | 1024MB DDR3-1333 (PC3-10600) SDRAM
| Manufacturer | Kingston
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 9.0 (Cycle Time: 1.500ns/686MHz)
| CAS# Latency | 8.0 (Cycle Time: 1.371ns/610MHz)
| CAS# Latency | 7.0 (Cycle Time: 1.200ns/533MHz)
| CAS# Latency | 6.0 (Cycle Time: 1.029ns/457MHz)
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.5 V
| Max Case Temperature | 95 °C (203 °F)
| SPD Revision | 1.0
| Part Number | 9905402-015.A03LF
| Manufacturing Location | China
| Manufacture Date | June 2009 (0926h)
| Serial Number | 14CC41B4h
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Not Supported
| Memory Slot 2
| Memory Type | 1024MB DDR3-1333 (PC3-10600) SDRAM
| Manufacturer | Kingston
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 9.0 (Cycle Time: 1.500ns/686MHz)
| CAS# Latency | 8.0 (Cycle Time: 1.371ns/610MHz)
| CAS# Latency | 7.0 (Cycle Time: 1.200ns/533MHz)
| CAS# Latency | 6.0 (Cycle Time: 1.029ns/457MHz)
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.5 V
| Max Case Temperature | 95 °C (203 °F)
| SPD Revision | 1.0
| Part Number | 9905402-015.A03LF
| Manufacturing Location | China
| Manufacture Date | June 2009 (0926h)
| Serial Number | 16CC37B4h
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Not Supported
Memory (SMBIOS)
| Physical Memory Array 1
| Maximum Capacity | 16384 MB
| Location | System Board or Motherboard
| Use | System Memory
| Memory Error Correct. | None
| Memory Devices | 4
| Structure Length | 0Fh
| Memory Device 1
| Size | 1024 MB
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1333 MHz
| Device Locator | A0
| Bank Locator | Bank0/1
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
| Memory Device 2
| Size | 1024 MB
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1333 MHz
| Device Locator | A1
| Bank Locator | Bank2/3
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
| Memory Device 3
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1333 MHz
| Device Locator | A2
| Bank Locator | Bank4/5
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
| Memory Device 4
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1333 MHz
| Device Locator | A3
| Bank Locator | Bank6/7
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
HDD
| Tertiary/Slave HDD
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA/ATAPI-7
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| HDD Marketing Size | 1000204 MB (1000.20 GB)
| Buffer Size | 32767.5 kB
| Buffer Type | Not Specified
| HDD Temperature | 44 °C (111 °F)
| Reallocated Sectors | 0
| HDD Health Status | Good
| ECC bytes | 50
| Security Erase Time | 194 min
| Enh. Security Erase | 194 min
| Current APM Value | None
| Acoustic Management | FEh (80h Recommended) - Disabled
| Access Method | 1
| ATA Controller Vendor | ATI Technologies Inc
| ATA Controller Name | SB700 SATA Controller [IDE mode]
| Device Location | Tertiary/Slave
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 6 (UltraDMA/133)
| Sectors per Interrupt | 16, Active: 16
| HDD Features
| SATA NCQ Command | Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Not Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Supported, Disabled
| Set Features Req. to Spinup | Supported, Enabled
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Supported, Disabled
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Supported, Enabled
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 51 | 200 | 200 | 0
| 3 | Spin-up Time | 21 | 253 | 253 | 6058
| 4 | Start/Stop Count | 0 | 95 | 95 | 5144
| 5 | Reallocated Sectors Count | 140 | 200 | 200 | 0
| 7 | Seek Error Rate | 51 | 200 | 200 | 0
| 9 | Power On Hours Count | 0 | 85 | 85 | 11226
| 10 | Spin-up Retry Count | 51 | 100 | 100 | 0
| 11 | Recalibration Retries | 51 | 100 | 100 | 0
| 12 | Drive Power Cycle Count | 0 | 95 | 95 | 5107
| 192 | Power-Off Retract Cycle | 0 | 198 | 198 | 1518
| 193 | Load/Unload Cycle Count | 0 | 199 | 199 | 5144
| 194 | Drive Temperature | 0 | 94 | 106 | 44
| 196 | Reallocation Event Count | 0 | 200 | 200 | 0
| 197 | Current Pending Sectors | 0 | 200 | 200 | 0
| 198 | Uncorrectable Sectors | 0 | 200 | 200 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 200 | 200 | 301
| 200 | Write Error Rate | 51 | 200 | 200 | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | WDC WD1001FALS-00J7B0 ATA Device
| Device Class | DiskDrive
| Device Location | Channel 0, Target 1, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7600.16385
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | IDE\DiskWDC_WD1001FALS-00J7B0___________________05.00K05
| Compatible ID | GenDisk
ATAPI
| ATAPI
| ATAPI Model | _NEC DVD_RW ND-3550A
| ATAPI Type | DVD+-RW DL/CD-RW
| Interface Type | Parallel ATA
| Physical Interface | ATAPI
| ATAPI Name | _NEC DVD_RW ND-3550A
| Vendor Specific | 05093000
| CD Read Speed | 48x (Current: 48x)
| CD Write Speed | 48x (Current: 48x)
| DVD Read Speed | Current: 6x
| DVD Write Speed | Current: 6x
| Buffer Size | 2048 kB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 15
| Write Retry Count | 0
| Compatibility | Unknown
| Serial Number | 63E1J06S211
| Controller Revision | 1.05
| Command DRQ Type | Microprocessor DRQ
| Command Packet Size | 12 bytes
| ATA Controller Vendor | ATI Technologies Inc
| ATA Controller Name | SB700 IDE
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 2 (UltraDMA/33), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Supported
| DVD-RAM Disk Read | Not Supported
| DVD-R Disk Read | Supported
| DVD-R DL Disk Read | Supported
| DVD-RW Disk Read | Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Supported
| DVD+R DL Disk Read | Supported
| DVD+RW Disk Read | Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Supported
| DVD-R DL Disk Write | Supported
| DVD-RW Disk Write | Supported
| DVD+R Disk Write | Supported
| DVD+R DL Disk Write | Supported
| DVD+RW Disk Write | Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Not Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Not Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard CD-ROM drives)
| Device Description | CD-ROM Drive
| Friendly Name | _NEC DVD_RW ND-3550A ATA Device
| Device Class | CDROM
| Device Location | Channel 0, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | cdrom.inf
| Service Name | cdrom
| Hardware ID | IDE\CdRom_NEC_DVD_RW_ND-3550A____________________1.05____
| Compatible ID | GenCdRom
| ATAPI
| ATAPI Model | CD-W540E
| ATAPI Type | CD-RW
| Interface Type | Parallel ATA
| Physical Interface | ATAPI
| ATAPI Name | TEAC CD-W540E
| Vendor Specific | 09/30/02
| CD Read Speed | 48x (Current: 48x)
| CD Write Speed | 40x (Current: 40x)
| Buffer Size | 8192 kB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 5
| Write Retry Count | 3
| Compatibility | ATA/ATAPI-5 revision 19
| Serial Number |
| Controller Revision | 1.0H
| Command DRQ Type | Accelerated DRQ
| Command Packet Size | 12 bytes
| ATA Controller Vendor | ATI Technologies Inc
| ATA Controller Name | SB700 IDE
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | 2, Active: None
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 2 (UltraDMA/33), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Not Supported
| DVD-RAM Disk Read | Not Supported
| DVD-R Disk Read | Not Supported
| DVD-R DL Disk Read | Not Supported
| DVD-RW Disk Read | Not Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Not Supported
| DVD+R DL Disk Read | Not Supported
| DVD+RW Disk Read | Not Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Not Supported
| DVD-R DL Disk Write | Not Supported
| DVD-RW Disk Write | Not Supported
| DVD+R Disk Write | Not Supported
| DVD+R DL Disk Write | Not Supported
| DVD+RW Disk Write | Not Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Not Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| S.M.A.R.T. | Not Supported
| S.M.A.R.T. Self-test | Not Supported
| S.M.A.R.T. Error Logging | Not Supported
| Security Mode Feature Set | Not Supported
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Supported, Enabled
| Write Cache | Not Supported
| Look-ahead | Not Supported
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Supported, Enabled
| Host Protected Area | Not Supported
| Write Verify Command | Not Supported
| Write Buffer Command | Not Supported
| Read Buffer Command | Not Supported
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Not Supported
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Not Supported
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Not Supported
| Device Configuration Overlay | Not Supported
| Flush Cache Command | Not Supported
| Flush Cache Ext Command | Not Supported
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Not Supported
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard CD-ROM drives)
| Device Description | CD-ROM Drive
| Friendly Name | TEAC CD-W540E ATA Device
| Device Class | CDROM
| Device Location | Channel 0, Target 1, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | cdrom.inf
| Service Name | cdrom
| Hardware ID | IDE\CdRomTEAC_CD-W540E___________________________1.0H____
| Compatible ID | GenCdRom
Storage (ASPI)
| Host: 0, Target: 1, LUN: 0
| Device Name | Kingston DT 101 II
| Size | 3874 MB (3.78 GB)
| Device Type | Disk Drive
| Compatibility | Not Standard
| Vendor Specific |
| Read Retry Count | 48
| Serial Number |
| Controller Revision | PMAP
| HDD Marketing Size | 4062 MB (4.06 GB)
| Location | Host: 0, Target: 1, LUN: 0
| Bus Width | 8-bit
| Address Width | 8-bit
| ASPI Device Features
| Removable Medium | Yes
| Read Cache | Not Supported
| Write Cache | Not Supported
| Read Reallocate | Not Supported
| Write Reallocate | Not Supported
| Terminate I/O Process | Not Supported
| Normal ACA | Not Supported
| Hierarchical Support | Not Supported
| Embedded Array Controller | Not Supported
| Protection Information | Not Supported
| Enclosure Services | Not Supported
| Multi-Ported Device | Not Supported
| Medium Changer | Not Supported
| Relative Addressing | Not Supported
| Synchronous Transfer | Not Supported
| Linked Commands | Not Supported
| Soft Reset | Not Supported
| Quick Arbitration | Not Supported
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | Kingston DT 101 II USB Device
| Device Class | DiskDrive
| Driver Provider | Microsoft
| Driver Version | 6.1.7600.16385
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | USBSTOR\DiskKingstonDT_101_II_______PMAP
| Compatible ID | USBSTOR\Disk
Logical Drives
| Local Drives
| A:
| Drive Letter | A:
| Drive Type | Floppy 1.44 MB (3.5")
| C:[SYSTEM]
| Drive Letter | C:
| Drive Type | Fixed Disk
| Volume Label | SYSTEM
| File System | FAT
| Volume Serial Number | 2255-1BEA
| Total Size | 2047.0 MB
| Free Space | 435.7 MB (21.3%)
| D:[UTILITIES]
| Drive Letter | D:
| Drive Type | Fixed Disk
| Volume Label | UTILITIES
| File System | FAT
| Volume Serial Number | 2E4A-1BEB
| Total Size | 2047.1 MB
| Free Space | 38.4 MB (1.9%)
| E:[GAMES]
| Drive Letter | E:
| Drive Type | Fixed Disk
| Volume Label | GAMES
| File System | FAT
| Volume Serial Number | 2D54-1BEC
| Total Size | 2047.1 MB
| Free Space | 491.5 MB (24.0%)
| F:[INSTALL]
| Drive Letter | F:
| Drive Type | Fixed Disk
| Volume Label | INSTALL
| File System | FAT32
| Volume Serial Number | 146C-1611
| Total Size | 70.3 GB
| Free Space | 2.6 GB (3.6%)
| G:[MUSIC]
| Drive Letter | G:
| Drive Type | Fixed Disk
| Volume Label | MUSIC
| File System | NTFS
| Volume Serial Number | D84A-C894
| Total Size | 815.2 GB
| Free Space | 5.4 GB (0.7%)
| H:[WINXP]
| Drive Letter | H:
| Drive Type | Fixed Disk
| Volume Label | WINXP
| File System | NTFS
| Volume Serial Number | 58B2-C918
| Total Size | 20.0 GB
| Free Space | 5.4 GB (26.8%)
| I:[SEVEN]
| Drive Letter | I:
| Drive Type | Fixed Disk
| Volume Label | SEVEN
| File System | NTFS
| Volume Serial Number | 10DE-1ECE
| Total Size | 20.0 GB
| Free Space | 2000.2 MB (9.8%)
| J:
| Drive Letter | J:
| Drive Type | Optical Drive
| K:
| Drive Letter | K:
| Drive Type | Optical Drive
| L:[KINGSTON]
| Drive Letter | L:
| Drive Type | Removable Disk
| Volume Label | KINGSTON
| File System | FAT32
| Volume Serial Number | AC1A-AC61
| Total Size | 3.8 GB
| Free Space | 3.8 GB (99.5%)
USB Devices
| USB Device 1
| Vendor (0951h) | Kingston Technology
| Device (1613h) | Data Traveler 8GB Pen Drive
| Manufacturer | Kingston
| Product | DT 101 II
| Serial Number | 0019E06B07EE5B8B0C020076
| Device Version | 1.00
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Bulk
| Data Packet Size | 64 bytes
| Max Power | 200 mA
| Driver
| Driver Status | The device is working properly
| Manufacturer | Compatible USB storage device
| Device Description | USB Mass Storage Device
| Device Class | USB
| Device Location | Port_#0006.Hub_#0003
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | usbstor.inf
| Service Name | USBSTOR
| Hardware ID | USB\VID_0951&PID_1613&REV_0100
| Compatible ID | USB\Class_08&SubClass_06&Prot_50
| Interface 1
| Class (08h) | Mass Storage
| SubClass (06h) | SCSI
| Protocol (50h) | Bulk (Zip)
| Interface |
| USB Device 2
| Vendor (046Dh) | Logitech
| Device (C05Ah) | USB Optical Mouse
| Manufacturer | Logitech
| Product | USB Optical Mouse
| Serial Number |
| Device Version | 54.00
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Interrupt
| Data Packet Size | 8 bytes
| Max Power | 98 mA Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | Port_#0003.Hub_#0005
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_046D&PID_C05A&REV_5400
| Compatible ID | USB\Class_03&SubClass_01&Prot_02
| Interface 1
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (02h) | Mouse
| Interface |
Physical Printers
| LPT/PnP or USB printer not found
Installed Printers
| Local Printers
| Installed Printer 1
| Printer Name | Microsoft XPS Document Writer
| Printer Port | XPSPort:
| Default Printer | Yes
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
| Installed Printer 2
| Printer Name | Fax
| Printer Port | SHRFAX:
| Default Printer | No
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
Slots (SMBIOS)
| Slot PCI
| Slot Type | PCI
| Current Usage | Available
| Data Bus Width | 32 bit
| Slot Designation | PCI
| Slot Length | Long Length
| Slot ID | 7
| Slot PCI
| Slot Type | PCI
| Current Usage | In Use
| Data Bus Width | 32 bit
| Slot Designation | PCI
| Slot Length | Long Length
| Slot ID | 6
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | Unknown
| Data Bus Width | 16x or x16
| Slot Designation | PCI Express x16
| Slot Length | Other
| Slot ID | 0
Ports (SMBIOS)
| Port 1 Other
| Int. Connector Type | On Board IDE
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | PRIMARY IDE
| Ext. Designator |
| Port 2 8251 FIFO Compatible
| Int. Connector Type | On Board Floppy
| Ext. Connector Type | None
| Port Type | 8251 FIFO Compatible
| Int. Designator | FDD
| Ext. Designator |
| Port 3 Serial Port 16450 Compatible
| Int. Connector Type | 9 Pin Dual Inline (pin 10 cut)
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16450 Compatible
| Int. Designator | COM1
| Ext. Designator |
| Port 4 Serial Port 16450 Compatible
| Int. Connector Type | 9 Pin Dual Inline (pin 10 cut)
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16450 Compatible
| Int. Designator | COM2
| Ext. Designator |
| Port 5 Parallel Port ECP/EPP
| Int. Connector Type | DB-25 pin female
| Ext. Connector Type | DB-25 pin female
| Port Type | Parallel Port ECP/EPP
| Int. Designator | LPT1
| Ext. Designator |
| Port 6 Keyboard Port
| Int. Connector Type | Other
| Ext. Connector Type | PS/2
| Port Type | Keyboard Port
| Int. Designator | Keyboard
| Ext. Designator |
| Port 7 Mouse Port
| Int. Connector Type | PS/2
| Ext. Connector Type | PS/2
| Port Type | Mouse Port
| Int. Designator | PS/2 Mouse
| Ext. Designator | No Detected
| Port 8 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 9 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 10 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 11 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 12 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 13 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 14 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 15 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 16 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 17 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 18 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 19 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
Network
| Network
| Network Name | A2KKV_7
| User Name | kkv1
| User Role | Administrator
| Logon Domain | A2KKV_7
| Interface 1
| Adapter Vendor | Realtek Semiconductor
| Adapter Name | RTL8168/8111 PCI-E Gigabit Ethernet NIC
| Subsys Vendor | Giga-Byte Technology
| Subsystem ID | GA-EP45-DS5 Motherboard
| Bus Type | PCI-E
| Description | Realtek RTL8168C(P)/8111C(P) Family PCI-E Gigabit Ethernet NIC (NDIS 6.20)
| MAC Address | 00-24-1D-89-15-40
| Adapter Type | Ethernet
| Link Speed | 100.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Operational
| DHCP Server | 192.168.1.1
| IP Address | 192.168.1.141
| IP Address Subnet Mask | 255.255.255.0
| Gateway | 192.168.1.1
| DNS Server | 192.168.1.1
| Interface 2
| Description | VMware Virtual Ethernet Adapter for VMnet1
| MAC Address | 00-50-56-C0-00-01
| Adapter Type | Ethernet
| Link Speed | 100.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Operational
| DHCP Enabled | No
| IP Address | 192.168.62.1
| IP Address Subnet Mask | 255.255.255.0
| Gateway | 0.0.0.0
| Interface 3
| Description | VMware Virtual Ethernet Adapter for VMnet8
| MAC Address | 00-50-56-C0-00-08
| Adapter Type | Ethernet
| Link Speed | 100.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Operational
| DHCP Enabled | No
| IP Address | 192.168.126.1
| IP Address Subnet Mask | 255.255.255.0
| Gateway | 0.0.0.0
Monitor
| Monitor
| Monitor Vendor | LG Electronics Inc.
| Monitor Model | LG FLATRON F920P
| Viewable Size | 17.7" (45.0 sm)
| Serial Number | 319823
| Manufacture Date | March 2005
| EDID Version | 1.3
| Monitor ID | GSM4A88
| Aspect Ratio | 4:3
| Horizontal Size | 36 sm
| Vertical Size | 27 sm
| Gamma Factor | 2.910
| Display Type | RGB Color
| Input Signal | Analog
| Internal Model | F920P
| Vertical Frequency | 50-160 Hz
| Horizontal Frequency | 30-111 kHz
| DPMS Features
| Active Off | Supported
| Suspend | Supported
| Standby | Supported
| Supported Modes
| Mode 1 | 720x400 @ 70 Hz (VGA)
| Mode 2 | 720x400 @ 88 Hz (XGA2)
| Mode 3 | 640x480 @ 60 Hz (VGA)
| Mode 4 | 640x480 @ 67 Hz (Mac II)
| Mode 5 | 640x480 @ 72 Hz (VESA)
| Mode 6 | 640x480 @ 75 Hz (VESA)
| Mode 7 | 800x600 @ 56 Hz (VESA)
| Mode 8 | 800x600 @ 60 Hz (VESA)
| Mode 9 | 800x600 @ 72 Hz (VESA)
| Mode 10 | 800x600 @ 75 Hz (VESA)
| Mode 11 | 832x624 @ 75 Hz (Mac II)
| Mode 12 | 1024x768 @ 87 Hz (interlaced)
| Mode 13 | 1024x768 @ 60 Hz (VESA)
| Mode 14 | 1024x768 @ 70 Hz (VESA)
| Mode 15 | 1024x768 @ 75 Hz (VESA)
| Mode 16 | 1280x1024 @ 75 Hz (VESA)
| Mode 17 | 1920x1440 @ 70 Hz
| Mode 18 | 2048x1536 @ 60 Hz
| Mode 19 | 1024x768 @ 85 Hz
| Mode 20 | 1280x1024 @ 75 Hz
| Mode 21 | 1280x1024 @ 85 Hz
| Mode 22 | 1600x1200 @ 75 Hz
| Mode 23 | 1600x1200 @ 85 Hz
| Mode 24 | 1152x864 @ 75 Hz
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard monitor types)
| Device Description | Generic PnP Monitor
| Device Class | Monitor
| Driver Provider | Microsoft
| Driver Version | 6.1.7600.16385
| Driver Date | 6-21-2006
| Inf File | monitor.inf
| Service Name | monitor
| Hardware ID | MONITOR\GSM4A88
| Compatible ID | *PNP09FF
Video
| Video
| Video Chip Vendor | ATI Technologies Inc
| Video Chip | RV770 [Radeon HD 4870]
| Subsystem Vendor | Hightech Information System Ltd (Medion??)
| Video Memory Size | 512 MB
| Video BIOS Version | 011.010.000.002
| Video BIOS Date | 2009/01/05 02:52
| Part Number | 113-BA0701-X07
| Core Temperature | 54 °C (129 °F)
| Current Core Clock | 300 MHz
| Current Memory Clock | 225 MHz
| Core Voltage | 1.083 V
| Core Usage | 0 %
| Performance Level | 0
| Bus Type | PCI-E
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 5.0 GB/s (Current: 5.0 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices, Inc.
| Device Description | ATI Radeon HD 4800 Series
| Device Class | Display
| Device Location | PCI bus 1, device 0, function 0
| Driver Provider | Advanced Micro Devices, Inc.
| Driver Version | 8.950.0.0
| Driver Date | 2-14-2012
| Inf File | oem3.inf
| Service Name | amdkmdap
| Hardware ID | PCI\VEN_1002&DEV_9440&SUBSYS_22671787&REV_00
| Compatible ID | PCI\VEN_1002&DEV_9440&REV_00
Hardware Monitoring
| Processor
| Processor | AMD Phenom II X3 710 2600 MHz
| Core Voltage | 1.050 V
| Core 1
| Temperature Core | 39 °C (102 °F)
| Core Clock | 803.6 MHz (Original: 2600 MHz)
| FSB Clock | 200.9 MHz
| Multiplier | 4.0
| Core 2
| Temperature Core | 39 °C (102 °F)
| Core Clock | 1406.4 MHz (Original: 2600 MHz)
| FSB Clock | 200.9 MHz
| Multiplier | 7.0
| Core 3
| Temperature Core | 39 °C (102 °F)
| Core Clock | 803.6 MHz (Original: 2600 MHz)
| FSB Clock | 200.9 MHz
| Multiplier | 4.0
| Video Card
| Video Chip | RV770 [Radeon HD 4870]
| Core Temperature | 55 °C (131 °F)
| Current Core Clock | 300 MHz
| Current Memory Clock | 225 MHz
| Core Voltage | 1.083 V
| Core Usage | 0 %
| Performance Level | 0
| Disk Drive
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Temperature | 44 °C (111 °F)
Drivers Troubleshooter
| List of Problem Devices
| Problem Device 1
| Device Type | PCI/AGP Device
| Vendor (1102h) | Creative Labs
| Device (0004h) | EMU10K2 Audio Chipset (SB Audigy Series)
| Subsys Vendor (1102h) | Creative Labs
| Subsystem ID (2005h) | Unknown
| Class (04h) | Multimedia
| SubClass (01h) | Audio
| Revision | 04h
| Driver Status | The device is disabled (22)
| Manufacturer | Creative Technology, Ltd.
| Device Description | Creative Audigy Audio Processor (WDM)
| Friendly Name | Creative SB Audigy 2 ZS (WDM)
| Device Class | MEDIA
| Device Location | PCI bus 3, device 6, function 0
| Driver Provider | Creative
| Driver Version | 6.0.1.1377
| Driver Date | 3-18-2010
| Inf File | oem2.inf
| Service Name | ctaud2k
| Hardware ID | PCI\VEN_1102&DEV_0004&SUBSYS_20051102&REV_04
| Compatible ID | PCI\VEN_1102&DEV_0004&REV_04
HDD Diagnostics
| HDD 1 Status
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| HDD Marketing Size | 1000204 MB (1000.20 GB)
| Buffer Size | 32767.5 kB
| ATA Controller Vendor | ATI Technologies Inc
| ATA Controller Name | SB700 SATA Controller [IDE mode]
| Device Location | Tertiary/Slave
| HDD Temperature | 44 °C (111 °F)
| Reallocated Sectors | 0
| HDD Health Status | Good
Windows
| Windows
| Operating System | MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
| OS Language | English (United States)
| Windows Folder | I:\Windows
| Kernel Type | Multiprocessor Free
| Registered Owner | Microsoft
| Registered Organization | Microsoft
| System UpTime | 0 Hour(s) 18 Minutes 53 Seconds
| IE Version | 8.0.7601.17514
| DirectX Version | DirectX 9.0c (4.09.00.0904)
| Regional Settings
| Country | Russia
| Language | Russian
| Time Zone | Azerbaijan Standard Time (GMT+4)
| Currency Name | Russian Ruble
| Measurment System | Metric
| ANSI Code Page | 1251
| OEM Code Page | 866
Installed Programs
| Installed Programs
| Adobe Systems Incorporated Adobe Flash Player 11 Plugin v11.1.102.63
| Sysinfo Lab ASTRA32 - Advanced System Information Tool 3.00
| Creative Technology Limited Creative Audio Console v1.33