Default modulation speed: Lower values mean that the vibrato will be slower, i.e. take more time to complete a full cycle of low-high-low. This affects both manual modulation (CC #1) and auto modulation (applied by some instruments). MIDIs can change this using NRPN H001.L008 or SysEx messages.