C  Data type 1: Project data
C
 1  1                                       9/06/2008             00000020000000
 1  2   C:\CDInstall2\Program files\BERS41\Data\Climate\climat17.TXT
 1  3    -33.9 151.2 150.0
 1  4  1C:\CDInstall2\Program files\BERS41\data\windowdata\BERSwindows.BWG
 1  6  1C:\CDInstall2\Program files\BERS41\data\windowdata\BERSskylights.BSG
 1  7   output.txt
 1  9   C:\CDInstall2\Program files\BERS41\temperature\accred13.TEM
 1 10   energy.txt
 1 11   airflow.txt
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C Basic data for ventilation modelling and numerics
C         MaxItV  MaxIVI   ConvV  ConvVI    UrfV  RungeK  MaxItT   ConvT  MaxItG   ConvG    UrfT
 1 12        100     100 0.00100 0.01000    0.20       5     100 0.10000     100 0.00100    0.20
C Cp data
 1 13  1  0.11  0.54  0.51  0.03 -0.62 -0.31 -0.33 -0.60
 1 13  2  0.50 -0.14 -0.71 -0.30 -0.33 -0.74 -0.03  0.53
 1 13  3 -0.33 -0.74 -0.03  0.53  0.50 -0.14 -0.71 -0.30
 1 13  4 -0.62 -0.31 -0.33 -0.60  0.11  0.54  0.51  0.03
C Shielding factor
 1 14     0.57
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C Ground model data
C Ground refl, sog area, perim, wall thick, conductance, diffusivity, edge insul, cond fl area
 1 15      0.2   166    58   0.2   1.5   4.6  0.00   143
C Curtain data for windows, maximum 20
C       AddedR Trans   Abs
C Holland Blind
 1 16  1  0.03  0.20  0.30
C Curtain data for roof windows (AddedR, Trans, Abs). 20 maximum
C 17 Not used
C Outdoor blinds shading factor for windows. 999 maximum
C Outdoor blinds shading factor for skylights and roof windows. 999 maximum
C 19 Not used
C Horizontal shading schemes. 999 maximum
C Scheme no., eave proj., eave offset, pergola proj, pergola offset, pergola shading factors
C        EaveP EaveO PergP PergO
 1 20  1  4.40  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  2  0.90  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  3  6.00  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  4  2.10  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  5  0.80  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  6 12.20  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  7  0.70  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  8  2.80  0.00  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20  9  4.40 -0.20  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20 10  2.10 -0.20  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20 11  0.90 -0.20  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20 12  0.80 -0.20  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
 1 20 13  0.70 -0.20  0.00  0.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00  1.00
C Vertical shading schemes. 999 maximum
C Left proj., left offset, right proj., right offset
C        LeftP LeftORightPRightO
 1 21  1  0.00  0.00  1.60  0.00
 1 21  2  1.60  0.00  0.00  0.00
 1 21  3  0.70  0.00  2.80  0.00
C Screen schemes. 1-999 maximum
C Scheme no., screen height, width, dist, offset horiz, offset vert, shading factors
C       Height Width  Dist  OffH  OffV
C  Number of repeats of day 1, repeat flag, starting temp, grid size for shade calcs
 1 23       10     0 -99.0    40
C  Stickiness period for controlled openings, Cooling thermostat leeway,
 1 26        3   2.5
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Data type 2: Construction data
C Change material properties
 2     0   801     0  0.24  0.28     0   20mm gap, slope 25, emit 0.9 and 0.4
C                                             File     System FrameU FrameF FrameA
 2N   1 Window   Generics CSIRO  clear glass  Timber/uPVC          (CSIRO Generic 03)
 2  1    25   4                                  1CSI-05-002a   4.20   0.21   0.50
C                                             Type   File     System FrameU FrameF
 2N  21 External Wall  Metal Clad Cavity Panel  R 1 Bulk Insulation
 2 21    45   1508  40209  57 34  10
 2N  22 External Wall  External DoorSolid timber door
 2 22    49  40
 2N 111 InterZone Wall  Cavity Panel 75mm gap   No Insulation
 2111    34  10508  40 34  10
 2N  51 External Floor  Ceramic Tiles  Concrete Slab on Ground   No Insulation
 2 51   999   0 18 100209   0
 2N  52 External Floor  Carpet and Underlay  Concrete Slab on Ground   No Insulation
 2 52   999   0 18 100209  24
 2N  53 External Floor  80/20 Carpet/Ceramic  Concrete Slab on Ground   No Insulation
 2 53   999   0 18 100209   9
 2N  81 Reverse External Floor  Ceramic Tiles  Concrete Slab on Ground   No Insulation
 2 81   209   0 18 100999   0
 2N  82 Reverse External Floor  Carpet and Underlay  Concrete Slab on Ground   No Insulation
 2 82   209  24 18 100999   0
 2N  83 Reverse External Floor  80/20 Carpet/Ceramic  Concrete Slab on Ground   No Insulation
 2 83   209   9 18 100999   0
 2N  91 External Ceiling  Plasterboard  R 2 Bulk Insulation
 2 91   999   0209 114 34  10
 2N  61 Reverse External Ceiling  Plasterboard  R 2 Bulk Insulation
 2 61    34  10209 114999   0
 2N 101 Internal Ceiling  Timber Above Plasterboard   No Insulation
 2101    50  20529  90 34  10
 2N  71 Internal Floor  Timber Above Plasterboard   No Insulation
 2 71    34  10529  90 50  20
 2N  31 Roof  Corrugated Iron   Foil, Reflective Side Down, Anti-glare Up
 2 31    45   1801   0999   0
 2N  30 Floorspace Walls 19mm hardwood
 2 30    49  19
 2N 121 Floorspace convective, Air to ground
 2121   999   0912   0999   0
 2N 122 Floorspace convective, Air to underfloor
 2122   999   0913   0999   0
 2N 123 Floorspace radiant (NonReflective), Ground to floor 
 2123   999   0914   0999   0
 2N 124 Floorspace radiant (Reflective), Ground to floor 
 2124   999   0915   0999   0
 2N  50 Floor of above ground, Earth
 2 50   902   0999   0
 2N 125 Roofspace convective, Air to ceiling
 2125   999   0908   0999   0
 2N 126 Roofspace convective, Air to roof
 2126   999   0909   0999   0
 2N 127 Roofspace radiant (NonReflective), Roof to ceiling
 2127   999   0910   0999   0
 2N 128 Roofspace radiant (Reflective), Roof to ceiling
 2128   999   0911   0999   0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C Data Type 3: Zone information
C  Zone   1  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  1   Family Kitchen 125.40  0.26  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  1  1  1.20  1.45    65     9     0     0     0     0     0     1     0
 3  1  1  1.30  1.21    65     9     0     0     0     0     0     1     0
 3  1  1  2.14  1.81    65     9     0     0     0     0     0     1     0
 3  1  1  1.30  1.21    65     9     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  1 21  2.40  9.60 14.28    65  0.50  0.50  0.90     1     0     0     0     0  0.00     0
 3  1 21  2.40  4.00  9.60   335  0.50  0.50  0.90     2     0     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  1111 11.04  0.50     2  0.00
 3  1111  1.30  0.50    10  0.00
 3  1111  0.72  0.50     8  0.00
 3  1111  1.44  0.50     8  0.00
 3  1111  7.44  0.50     7  0.00
 3  1111  0.68  0.50     7  0.00
 3  1111  4.52  0.50     6  0.00
 3  1111  0.44  0.50     5  0.00
 3  1111  0.44  0.50     4  0.00
 3  1111  2.88  0.50     4  0.00
 3  1111  2.40  0.50     3  0.00
 3  1111  8.36  0.50     3  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  1 51 52.25  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  1 91 52.25  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  1300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  1301  0.15   0.6   100  0.90  2.10     1     1   0.5     0     0  0.00     0     0
 3  1302  0.12   0.6   100  0.80  2.10     1     1   0.5     0     0  0.00     0     0
 3  1303  0.18   0.6   100  0.00  2.14     1     1   0.5     0     0  0.00     0     0
 3  1304  0.12   0.6   100  0.80  2.10     1     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
 3  1305  0.75   0.6   100  0.00  2.10    -1     1   0.5    10     1  0.00     0     0
 3  1306  0.82   0.6   100  0.00  2.10    -1     1   0.5     7     1  0.00     0     0
 3  1307  0.82   0.6   100  0.00  2.10    -1     1   0.5     6     1  0.00     0     0
 3  1308  0.82   0.6   100  0.00  2.10    -1     1   0.5     5     1  0.00     0     0
 3  1309  0.82   0.6   100  0.00  2.10    -1     1   0.5     4     1  0.00     0     0
 3  1310  0.82   0.6   100  0.00  2.10    -1     1   0.5     3     1  0.00     0     0
C       Sensible internal heat gain (watts), [hours 1-12]
 3  1401   100   100   100   100   100   100   100   699   399   191   191   191
C       Sensible internal heat gain (watts), [hours 13-24]
 3  1402   191   191   191   191   191   431  1431   581   581   581   100   100
C       Latent internal heat gain (watts), [hours 1-12]
 3  1403     0     0     0     0     0     0     0   351   151    76    76    76
C       Latent internal heat gain (watts), [hours 13-24]
 3  1404    76    76    76    76    76   114   714   114   114   114     0     0
C       Heating thermostat settings [hours 1-12]
 3  1501   0.0   0.0   0.0   0.0   0.0   0.0   0.0  20.0  20.0  20.0  20.0  20.0
C       Heating thermostat settings [hours 13-24]
 3  1502  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0
C       Cooling thermostat settings [hours 1-12]
 3  1503   0.0   0.0   0.0   0.0   0.0   0.0   0.0  25.5  25.5  25.5  25.5  25.5
C       Cooling thermostat settings [hours 13-24]
 3  1504  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  1601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  1603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  1604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  1605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   2  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  2   Dining lounge   73.97  0.26  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  2  1  1.30  1.45    65     9     0     0     0     0     0     1     0
 3  2  1  1.20  1.30   155    10     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  2 21  2.40  6.70 14.19    65  0.50  0.50  0.90     3     0     0     0     0  0.00     0
 3  2 21  2.40  4.60  9.48   155  0.50  0.50  0.90     4     0     0     0     0  0.00     0
 3  2 21  2.40  0.70  1.68   245  0.50  0.50  0.90     3     1     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  2111 14.40  0.50    10  0.00
 3  2111 11.04  0.50     1  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  2 52 30.82  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  2 91 30.82  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  2300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  2301  0.15   0.6   100  0.80  2.10     1     1   0.5     0     0  0.00     0     0
 3  2302  0.13   0.6   100  0.90  2.10     3     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
C       Sensible internal heat gain (watts), [hours 1-12]
 3  2401     0     0     0     0     0     0     0   177   177    54    54    54
C       Sensible internal heat gain (watts), [hours 13-24]
 3  2402    54    54    54    54    54   195   195   195   195   195     0     0
C       Latent internal heat gain (watts), [hours 1-12]
 3  2403     0     0     0     0     0     0     0    54    54    27    27    27
C       Latent internal heat gain (watts), [hours 13-24]
 3  2404    27    27    27    27    27    40    40    40    40    40     0     0
C       Heating thermostat settings [hours 1-12]
 3  2501   0.0   0.0   0.0   0.0   0.0   0.0   0.0  20.0  20.0  20.0  20.0  20.0
C       Heating thermostat settings [hours 13-24]
 3  2502  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0  20.0
C       Cooling thermostat settings [hours 1-12]
 3  2503   0.0   0.0   0.0   0.0   0.0   0.0   0.0  25.5  25.5  25.5  25.5  25.5
C       Cooling thermostat settings [hours 13-24]
 3  2504  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  2601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  2603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  2604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  2605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   3  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  3   Laundry         17.28  1.43  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  3  1  2.14  1.57   335    11     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  3 21  2.40  2.20  1.92   335  0.50  0.50  0.90     2     0     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  3111  8.36  0.50     1  0.00
 3  3111  2.40  0.50     1  0.00
 3  3111  4.08  0.50     4  0.00
 3  3111  2.88  0.50     4  0.00
 3  3111  6.00  0.50     5  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  3 51  7.20  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  3 91  7.20  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  3300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  3301  0.63   0.6   100  0.00  2.14     2     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
 3  3302  0.82   0.6   100  0.00  2.10    -1     1   0.5     1     1  0.00     0     0
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  3601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  3603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  3604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  3605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   4  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  4   WC               4.90  4.22  0.03  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  4111  0.44  0.50     1  0.00
 3  4111  1.92  0.50     5  0.00
 3  4111  2.88  0.50     3  0.00
 3  4111  4.08  0.50     3  0.00
 3  4111  2.88  0.50     1  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  4 51  2.04  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  4 91  2.04  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  4300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
C External door ventilation
C Internal door ventilation
 3  4301  0.82   0.6   100  0.00  2.10    -1     1   0.5     1     1  0.00     0     0
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  4601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  4603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  4604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  4605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   5  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  5   Bedroom 4       28.51  0.26  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  5  1  1.30  1.45   335    11     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  5 21  2.40  3.30  7.92   245  0.50  0.50  0.90     5     0     0     0     0  0.00     0
 3  5 21  2.40  3.60  6.75   335  0.50  0.50  0.90     2     0     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  5111  6.00  0.50     3  0.00
 3  5111  1.92  0.50     4  0.00
 3  5111  0.44  0.50     1  0.00
 3  5111  6.48  0.50     6  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  5 52 11.88  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  5 91 11.88  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  5300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  5301  0.15   0.6   100  0.80  2.10     2     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
 3  5302  0.82   0.6   100  0.00  2.10    -1     1   0.5     1     1  0.00     0     0
C       Sensible internal heat gain (watts), [hours 1-12]
 3  5401    30    30    30    30    30    30    30     0     0     0     0     0
C       Sensible internal heat gain (watts), [hours 13-24]
 3  5402     0     0     0     0     0     0     0    15    15    15    44    30
C       Latent internal heat gain (watts), [hours 1-12]
 3  5403    15    15    15    15    15    15    15     0     0     0     0     0
C       Latent internal heat gain (watts), [hours 13-24]
 3  5404     0     0     0     0     0     0     0     0     0     0    15    15
C       Heating thermostat settings [hours 1-12]
 3  5501  15.0  15.0  15.0  15.0  15.0  15.0  15.0  18.0  18.0   0.0   0.0   0.0
C       Heating thermostat settings [hours 13-24]
 3  5502   0.0   0.0   0.0   0.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0
C       Cooling thermostat settings [hours 1-12]
 3  5503  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5   0.0   0.0   0.0
C       Cooling thermostat settings [hours 13-24]
 3  5504   0.0   0.0   0.0   0.0  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  5601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  5603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  5604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  5605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   6  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  6   Bathroom        13.99  1.71  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  6  1  0.90  1.21   245    12     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  6 21  2.40  1.90  3.47   245  0.50  0.50  0.90     5     0     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  6111  4.52  0.50     1  0.00
 3  6111  2.40  0.50     7  0.00
 3  6111  1.68  0.50     7  0.00
 3  6111  4.08  0.50     7  0.00
 3  6111  6.48  0.50     5  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  6 51  5.83  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  6 91  5.83  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  6300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  6301  0.12   0.6   100  1.20  2.10     4     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
 3  6302  0.82   0.6   100  0.00  2.10    -1     1   0.5     1     1  0.00     0     0
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  6601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  6603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  6604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  6605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   7  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  7   Bedroom 3       30.38  0.26  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  7  1  1.30  1.45   245    12     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  7 21  2.40  3.80  7.23   245  0.50  0.50  0.90     5     0     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  7111  7.44  0.50     1  0.00
 3  7111  8.88  0.50     8  0.00
 3  7111  4.08  0.50     6  0.00
 3  7111  1.68  0.50     6  0.00
 3  7111  2.40  0.50     6  0.00
 3  7111  0.68  0.50     1  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  7 52 12.66  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  7 91 12.66  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  7300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  7301  0.15   0.6   100  0.80  2.10     4     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
 3  7302  0.82   0.6   100  0.00  2.10    -1     1   0.5     1     1  0.00     0     0
C       Sensible internal heat gain (watts), [hours 1-12]
 3  7401    32    32    32    32    32    32    32     0     0     0     0     0
C       Sensible internal heat gain (watts), [hours 13-24]
 3  7402     0     0     0     0     0     0     0    16    16    16    47    32
C       Latent internal heat gain (watts), [hours 1-12]
 3  7403    16    16    16    16    16    16    16     0     0     0     0     0
C       Latent internal heat gain (watts), [hours 13-24]
 3  7404     0     0     0     0     0     0     0     0     0     0    16    16
C       Heating thermostat settings [hours 1-12]
 3  7501  15.0  15.0  15.0  15.0  15.0  15.0  15.0  18.0  18.0   0.0   0.0   0.0
C       Heating thermostat settings [hours 13-24]
 3  7502   0.0   0.0   0.0   0.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0
C       Cooling thermostat settings [hours 1-12]
 3  7503  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5   0.0   0.0   0.0
C       Cooling thermostat settings [hours 13-24]
 3  7504   0.0   0.0   0.0   0.0  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  7601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  7603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  7604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  7605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   8  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  8   Bedroom 2       29.33  0.26  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  8  1  1.30  1.45   245    12     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  8 21  2.40  3.10  5.55   245  0.50  0.50  0.90     5     0     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  8111  1.44  0.50     1  0.00
 3  8111  0.72  0.50     1  0.00
 3  8111  4.28  0.50    10  0.00
 3  8111  9.60  0.50     9  0.00
 3  8111  8.88  0.50     7  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  8 52 12.22  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  8 91 12.22  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  8300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  8301  0.15   0.6   100  0.80  2.10     4     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
 3  8302  0.82   0.6   100  0.00  2.10    -1     1   0.5    10     1  0.00     0     0
C       Sensible internal heat gain (watts), [hours 1-12]
 3  8401    31    31    31    31    31    31    31     0     0     0     0     0
C       Sensible internal heat gain (watts), [hours 13-24]
 3  8402     0     0     0     0     0     0     0    15    15    15    46    31
C       Latent internal heat gain (watts), [hours 1-12]
 3  8403    15    15    15    15    15    15    15     0     0     0     0     0
C       Latent internal heat gain (watts), [hours 13-24]
 3  8404     0     0     0     0     0     0     0     0     0     0    15    15
C       Heating thermostat settings [hours 1-12]
 3  8501  15.0  15.0  15.0  15.0  15.0  15.0  15.0  18.0  18.0   0.0   0.0   0.0
C       Heating thermostat settings [hours 13-24]
 3  8502   0.0   0.0   0.0   0.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0
C       Cooling thermostat settings [hours 1-12]
 3  8503  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5   0.0   0.0   0.0
C       Cooling thermostat settings [hours 13-24]
 3  8504   0.0   0.0   0.0   0.0  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  8601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  8603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  8604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  8605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone   9  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3  9   Bedroom 1       56.64  0.26  0.09  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
 3  9  1  1.30  1.81   155    13     0     0     0     0     0     1     0
 3  9  1  0.90  1.05   245    12     0     0     0     0     0     1     0
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3  9 21  2.40  2.80  6.72    65  0.50  0.50  0.90     6     2     0     0     0  0.00     0
 3  9 21  2.40  3.60  6.29   155  0.50  0.50  0.90     7     0     0     0     0  0.00     0
 3  9 21  2.40  6.30 14.17   245  0.50  0.50  0.90     5     0     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3  9111  5.52  0.50    10  0.00
 3  9111  0.96  0.50    10  0.00
 3  9111  1.16  0.50    10  0.00
 3  9111  9.60  0.50     8  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3  9 53 23.60  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3  9 91 23.60  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3  9300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
 3  9301  0.18   0.6   100  0.80  2.10     3     1   0.5     0     0  0.00     0     0
 3  9302  0.11   0.6   100  1.20  2.10     4     1   0.5     0     0  0.00     0     0
C External door ventilation
C Internal door ventilation
 3  9303  0.82   0.6   100  0.00  2.10    -1     1   0.5    10     1  0.00     0     0
C       Sensible internal heat gain (watts), [hours 1-12]
 3  9401    59    59    59    59    59    59    59     0     0     0     0     0
C       Sensible internal heat gain (watts), [hours 13-24]
 3  9402     0     0     0     0     0     0     0    29    29    29    88    59
C       Latent internal heat gain (watts), [hours 1-12]
 3  9403    30    30    30    30    30    30    30     0     0     0     0     0
C       Latent internal heat gain (watts), [hours 13-24]
 3  9404     0     0     0     0     0     0     0     0     0     0    30    30
C       Heating thermostat settings [hours 1-12]
 3  9501  15.0  15.0  15.0  15.0  15.0  15.0  15.0  18.0  18.0   0.0   0.0   0.0
C       Heating thermostat settings [hours 13-24]
 3  9502   0.0   0.0   0.0   0.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0  18.0
C       Cooling thermostat settings [hours 1-12]
 3  9503  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5   0.0   0.0   0.0
C       Cooling thermostat settings [hours 13-24]
 3  9504   0.0   0.0   0.0   0.0  25.5  25.5  25.5  25.5  25.5  25.5  25.5  25.5
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3  9601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3  9603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3  9604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3  9605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C  Zone  10  Normal Zone
CZone              Name   Vol     A     B WsRed  Type EstSG
 3 10   Entrance        18.43  0.62  0.21  0.47Normal     1
C Windows
C       Height Width  AzimHSSch1HSSch2VShSchScSch1ScSch2ScSch3 Curtn Blind
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C External Walls
C       Height Width NArea  Azim  AbsO  AbsI EmissHShSchVShSchScSch1ScSch2ScSch3SHGFra
 3 10 21  2.40  1.60  2.12   155  0.50  0.50  0.90     8     3     0     0     0  0.00     0
 3 10 22  2.10  0.82  1.72   155  0.50  0.50  0.90     8     3     0     0     0  0.00     0
C Floors, Ceilings, Partitions
C Interzone Walls
C         Area  AbsI  AdjZ  SHGF
 3 10111 14.40  0.50     2  0.00
 3 10111  1.16  0.50     9  0.00
 3 10111  0.96  0.50     9  0.00
 3 10111  5.52  0.50     9  0.00
 3 10111  4.28  0.50     8  0.00
 3 10111  1.30  0.50     1  0.00
C Walls within zones
C         Area  AbsI  SHGF
C Walls adjacent to neighbour
C         Area  AbsI  SHGF
C Slab on Ground
C         Area  AbsI  AdjZ
 3 10 51  7.68  0.50    11
C Ceiling of habitable zone below roofspace
C         Area  AbsI  AdjZ
 3 10 91  7.68  0.50    14
C General ventilation data
C        FlrHtCeilHtMecSupMechEx
 3 10300  0.00  2.40   0.0   0.0
C Data for each ventilation opening
C    No. Width    Cd  Perc   Low  HighCpIndx  Type ExponAdjZonConTyp MidHtContrlLouvre
C Stair void ventilation
C Window ventilation
C External door ventilation
 3 10301  0.82   0.6   100  0.00  2.10     3     1   0.5     0     0  0.00     0     0
C Internal door ventilation
 3 10302  0.82   0.6   100  0.00  2.10    -1     1   0.5     9     1  0.00     0     0
 3 10303  0.82   0.6   100  0.00  2.10    -1     1   0.5     8     1  0.00     0     0
 3 10304  0.75   0.6   100  0.00  2.10    -1     1   0.5     1     1  0.00     0     0
C   Indoor covering closing & opening times, drawing temp, drawing solar for windows
 3 10601    18     7  28.0   200
C   External blind drawing temp, drawing solar for windows
 3 10603  25.0    75
C   External blind drawing temp, drawing solar for skylights
 3 10604  25.0    75
C   Ventilation on & off times, on & off temps, A factor, B factor
 3 10605     0    24  25.0  22.0   0.0   0.0
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C Zone  11 Under Slab
C                  Name   Vol     A     B WsRed  Type EstSG
 3 11     UnderSlab   1   0.0  0.00  0.00  0.47Normal     1
C Ceilings (Reverse Floor), Floor (Ground)
C         Area  AbsI  AdjZ
 3 11 81 52.25  0.50     1
 3 11 82 30.82  0.50     2
 3 11 81  7.20  0.50     3
 3 11 81  2.04  0.50     4
 3 11 82 11.88  0.50     5
 3 11 81  5.83  0.50     6
 3 11 82 12.66  0.50     7
 3 11 82 12.22  0.50     8
 3 11 83 23.60  0.50     9
 3 11 81  7.68  0.50    10
 3 11 50166.18  0.50
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C Zone  12 Roof Space
C                  Name   Vol     A     B WsRed  Type EstSG CeilZ RoofZ REmis
 3 12     Roofspace   1  22.9  2.00  1.00  0.47RoofSA     1    14    13  0.05
C Conv to Under-roof, Conv to Above Ceilings
C         Area  AbsI  AdjZ
 3 12126183.36  0.50    13
 3 12125166.18  0.50    14
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C Zone  13 Underside of Roof
C                  Name   Vol     A     B WsRed  Type EstSG
 3 13   UnderSideRf   1   0.0  0.00  0.00  0.47Normal     1
C Conv to Roofspace Air, Rad to Above Ceilings, Roof
C         Area  AbsI  AdjZ
 3 13126183.36  0.50    12
 3 13128166.18  0.50    14
C Skylights
C         Area  Azim Slope ShadI ShadEZonlit ShLenShAreaShRefl ShRes  Diff VArea VType
C Roofs
C         Area  Azim Slope  AbsE  AbsI Emiss SHGFra
 3 13 31183.36  0.00  0.00  0.45  0.45  0.90
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
C Zone  14 Top of Ceiling
C                  Name   Vol     A     B WsRed  Type EstSG
 3 14   TopOfCeiling  1   0.0  0.00  0.00  0.47Normal     1
C Floors(Reverse Ceilings), Conv to Roofspace, Rad to Under-roof
C         Area  AbsI  AdjZ
 3 14 61 52.25  0.50     1
 3 14 61 30.82  0.50     2
 3 14 61  7.20  0.50     3
 3 14 61  2.04  0.50     4
 3 14 61 11.88  0.50     5
 3 14 61  5.83  0.50     6
 3 14 61 12.66  0.50     7
 3 14 61 12.22  0.50     8
 3 14 61 23.60  0.50     9
 3 14 61  7.68  0.50    10
 3 14125166.18  0.50    12
 3 14128166.18  0.50    13
CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC
 9
