---Car---

Type 	  	Lamborghini
Murciélago
  	  	 
Base Price 	  	€ 223880
  	  	 
Manufacturer 	  	

Automobili Lamborghini SpA
Via Modena 12
40019 Sant' Agata- Bolognese
  	  	 
Website 	  	www.lamborghini.it


---Test---

Testing Date 	  	

6/2002
  	  	 
Temperature (Air) 	  	14 Degree Celsius
Temperature (Asphalt) 	  	11 Degree Celsius
Air Pressure 	  	1017 mbar
  	  	 
Defects during Test 	  	-


---Engine---

Displacement 	  	6192 cccm
Cylinders 	  	12
Valves 	  	48
Supercharger(s) 	  	-
Bore x Stroke 	  	87 x 86,8 mm
Compression Ratio 	  	10,7:1
Power 	  	580 Bhp (426 KW)
at 7500/min
Torque 	  	650 Nm
at 5400/min
Bhp / Liter 	  	93,7 PS / L

---Transmission---

Transmission Type 	  	Manual
Number of Gears 	  	6
Power Transmission 	  	all-wheel drive
Gear Ratio 	  	1,92

---Chassis / Body---

Length 	  	4580 mm
Width 	  	2045 mm
Height 	  	1135 mm
Wheel Base 	  	2665 mm
Tank Volume 	  	100 L
Weight 	  	1820 Kg
Weight Distribution 	  	783 Kg / 1037 Kg
43%/57%
  	  	 
Weight / Bhp	3,4 Kg / PS

---Wheels/ Tires---

Wheels (Front/Rear) 	  	8,5" / 13"
Tires 	  	Pirelli P Zero Rosso
Dimension Front 	  	245/35/18
Dimension Rear 	  	335/30/18

---Acceleration---          

0 - 40 Km/h 	  	1,2 s
0 - 60 Km/h 	  	1,9 s
0 - 80 Km/h 	  	2,7 s
0 - 100 Km/h 	  	3,9 s
0 - 120 Km/h 	  	5,3 s
0 - 140 Km/h 	  	6,6 s
0 - 160 Km/h 	  	8,9 s
0 - 180 Km/h 	  	10,6 s
0 - 200 Km/h 	  	12,8 s

---Top Speed--- 
         
Vmax 	  	330 Km/h

---Elasticity---

  	  	4.Gear 	  	5.Gear 	  	6.Gear
80 - 100 Km/h 	  2,8 s 		3,1 s 	  	3,8 s
80 - 120 Km/h 	  5,4 s 		6 s 	  	7,2 s
80 - 160 Km/h 	  10,2 s 		12,3 s 	  	14,9 s
80 - 180 Km/h 	  12,8 s 		15 s 	  	18,5 s
80 - 200 Km/h 	  	- s 	  	- s 	  	- s

---Braking---
  	  	
Distance
	  	
m/s2
100 - 0 Km/h cold 	  	35,4 m 	  	10,9
100 - 0 Km/h hot 	  	36,4 m 	  	10,6
200 - 0 Km/h 	  	139,1 m 	  	11,1
80% Vmax* - 0 Km/h 	  	- m 	  	-
  	  	  	  	 
200 - 0 Km/h 	  	5 s 	  	* 264 km/h

---Technology---

Type of Brake 	  	Scheiben
innenbelüftet und gelocht
  	  	 
Discs Ø Front 	  	355 mm
Discs Ø Rear 	  	355 mm
  	  	 
ABS 	  	Yes

---Wind Tunnel---

Buoyancy at 200 Km/h
(Rear Axis) 	  	-1 Kg
cw Value 	  	0,33

---Transverse Acceleration---

Maximum G-Force 	  	1,2 g
at Speed 	  	86 Km/h

---Acceleration/Braking---

0 - 200 - 0 Km/h 	  	17,8 s

---Handling---

Slalom Course (36m) 	  	124 Km/h
Evasive Course (110m)		138 Km/h

---Fuel consumption *---

Minimum 	  	15,6 L
Average 	  	20,8 L
Maximum 	  	31,2 L
  	  	 
* 98 Octane 	 

